

**Laboratory**

All reportable analytes

M08 – Master File Notification – Test/Observation

**Client**

Orderable group tests (Panels, Profiles, etc.)

M10 – Master File Notification – Test/Observation Batteries

Procedure Codes

M04 – Master File Notification – Charge Description

# Primary Keys Discussion

* MFE-4 Primary Key Value – MFE – currently repeats
  + Propose to constrain MFE-4 in eDOS R2 so the field does not repeat, however, the MFE segment "loop" can repeat
  + MFE-4 Primary Key Value – MFE (CWE\*) shall match OM1-2 Producer's Service/Test/Observation ID (CWE)
  + OM1-1, OM2-1, OM3-1, OM4-1, and OM5-1 Sequence Number - Test/Observation Master File must match within segment grouping per HL7 standard (NM data type)
  + CDM-1 (CWE) shall match OM1-2 Producer's Service/Test/Observation ID (CWE)
* OM4 segment repeats, contingent on OM1-4 (Specimen Required) =Y. Options to manage:
  + Leave OM4-1 as is matching OM1-1, for validation, check OM4-6 Specimen values be different
  + Format numbering OM4-1 in segment repetitions, which is a NM data type, as follows: 1.1, 1.2, 1.3, etc. (has to be approved by HL7 InM)

\*Generic CWE, vs. specific CWE flavor, used in these examples